**SPECIFICATION SHEET**

**PRODUCT NAME: 2\*RJ11 shutter**

**PRODUCT No.:**  **F100C**



ADD: 152 xinguang industrial zone, yueqing city, zhejiang province

（TEL）:0086-577-62799688

（E-mail）：info@safewirele.com

(WEB): http://www.safewirele.c

**Quick Details**

Place of Origin:Zhejiang, China

Brand Name:Safewrie

Model Number:F100C

Product Name:2\*RJ11 shutter

Color:White

Size: 45\*45mm

IDC:Phosphor Bronze,Tinplating

Connector Type:Modular

Usage:Telephone wire,network cable

Packing:Bag+Carton, Box+Carton

Certificate:RoHS ISO9001,ISO14001,OHSMS18001

Keywords:Keystone Jack,Modular

Type:2\*RJ11 shutter

**Product Show:**

****

**Products Featuer**

It is lead out from the RJ11 series ports which is suitable for the international standard;IDC or binding posts:Phosphor Bronze materials,tin plated,can contact with 22~26AWG solid wire;line 2,line 4,line 6:the thickness of gold-plating which on Phosphorus copper wire is 3µinch-50µinch;

**Electrical Performance**

1.Insulation resistance:no less than 1000MΩ

2.Withstand voltage strength:DC700V(AC500V)in 1 min

3.Contact resistance:no more than 30MΩ

**Mechanical performance**

Useful life:the times of insertion and extration is no less than 750,repetation time of terminal fixed line is no less than 80.

**Operating environment**

1.Operating temperature : -10~60 ℃

2.Operating humidity:10-90%

**RoHS Certificate of Compliance：**Conforms with the Directive 2002/95/EC (ROHS) regarding to limitation of dangerous substances,in particular to clause 4 which forbids the use of substances: