**SPECIFICATION SHEET**

**PRODUCT NAME: Male XLR/Canon solderless**

**PRODUCT No.:**  **F60-B**



ADD: 152 xinguang industrial zone, yueqing city, zhejiang province

（TEL）:0086-577-62799688

（E-mail）：info@safewirele.com

(WEB): http://www.safewirele.c

**Quick Details**

Place of Origin:Zhejiang, China

Brand Name:OEM

Model Number:F60-B

Type: modules socket

Grounding:Non-Grounding

Rated Voltage:110V-250V

Rated Current:depends on modular

Application:Residential / General-Purpose

Size:45\*22.5mm

Material:ABS

Module:network

Color:White

**Detail**

|  |  |
| --- | --- |
| Product size: | 45mm\*22.5mm |
| Material | ABS + Brass |
| ·Operating Voltage | AC 220V~250V/50HZ-60HZ |
| ·Energy Consumption | <0.1mA |
| ·Operating Environment | 30~70 Centigrade, less than 95%RH |
| ·Longevity | 100,000 times operation/ Two years warranty |
| Type | Male XLR/Canon solderless |

**Product Show:**

**Features:**

1. High grade fireproof PC material panel, high temperature resistance and durable.

2. Easy to install and safety

3. Ergonomics and modern industrial design bring you more soft, smooth feel

4. A good tool for structured cabling. For home and office DIY cabling.

5. Voltage: 220-250V, could be universal used for most countries.

6. OEM orders like printing logo are welcomed by us

*Application:*  
    They are mainly used mobile phone, CD machine, wireless phone, digital notebook computer, digital camera, TV, home appliance, audio-visual, film and television and so on.

**RoHS Certificate of Compliance：**Conforms with the Directive 2002/95/EC (ROHS) regarding to limitation of dangerous substances,in particular to clause 4 which forbids the use of substances: