
**SPECIFICATION SHEET**

**PRODUCT NAME: Switch sockets**

**PRODUCT No.:**  **F84**



ADD: 152 xinguang industrial zone, yueqing city, zhejiang province

（TEL）:0086-577-62799688

（E-mail）：info@safewirele.com

(WEB): http://www.safewirele.com

**Quick Details**

Place of Origin:Zhejiang, China

Brand Name:Safewire

Model Number：F84

Type：2 Gang 2 way switch

Max. Current:15A

Max. Voltage:120V

Mechanical Life:10 Years

Color:White


Net weight:150g

Working frequency:2.412~2.48MHz

**Describe**

|  |  |
| --- | --- |
| type | 2 gang 2 way switch |
| color | white |
| Shelf life | 5 years |
| Current | 10A |
| Voltage | 250V |
| Panel  Material | ABS |
| Inside Material | High quality brass and ABS |
| Size | 45\*45mm |
| Advantage | This is two way switch socket, that is more conducive to wiring |
| Type | Switch sockets |

**Product Show:**

****

1.Flame-retardant nylon is used in the backseat, strong flame-retardant

2.High elastic tin phosphor bronze is used for switch contact.

3.The surface material of the panel is made of ABS.

**Application**

The product use in floor box or desktop socket or the wall .

**RoHS Certificate of Compliance：**Conforms with the Directive 2002/95/EC (ROHS) regarding to limitation of dangerous substances,in particular to clause 4 which forbids the use of substances: