Wenzhou Safewire Electric CO.,Ltd.

**SPECIFICATION SHEET**

**PRODUCT NAME: Incline socket**

**PRODUCT No.:**  **FZ-1770**



Address:2nd floor, Wealth Garden, Liushi town, Yueqing, Wenzhou,China ,325604

Tel:0086-577-61725369

Mob:0086-18612380398

ZIP:325604

（E-mail）：info@safewirele.com

(WEB): http://www.safewirele.com

***Technical parameters & characteristic :***

1. ***Working environment:***
2. The environment temperature:-5℃~/40℃
3. The rated voltage：100V~~250V
4. Rated current：10A、13A、16A、20A
5. ***Characteristic:***

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| ****1**** | ****Model**** | ****FA-1770**** | ****6**** | ****HS Code**** | **8536690000** |
| ****2**** | ****Brand Name**** | **Safewire or OEM brand** | ****7**** | ****Market standard**** | ****Customized**** |
| ****3**** | ****Type**** | **Incline Socket** | ****8**** | ****Place of origin**** | **Zhejiang , Wenzhou, China** |
| ****4**** | ****Color**** | **White/black** | ****9**** | ****Frequency**** | **50Hz~60Hz** |
| ****5**** | ****Grounding**** | **Standard grounding** | ****10**** | ****Current Type**** | **AC** |

1. ***Technical parameters :***

|  |  |  |
| --- | --- | --- |
| **Serial No.** | **Parameter** | **Description** |
| **1** | **Panel Material** | **Fire-retarant ABS plastic** |
| **2** | **Capacity of modules /Interface size** | **2 ways (45\*45mm)modules** |
| **3** | **Configuration** | **1 Power socket or 1\* USB charger or 2 \*RJ45 Network** |
| **4** | **Available modules** | **45mm modules** |
| **5** | **Cable length** | **1.5m, 2m,2m or required length** |
| **6** | **Size** | **86.4\*115\*85** |
| **7** | **Installation** | **stand-alone** |

**Product show**



**Feature**

1. **Easy Access with 45 degree:**The socket design is vertical, and the socket is tilted at 45 degrees, which is helpful for customers to get power in the desktop.
2. **ABS Plastic:**Made of high temperature resistant, not easy to scratch ABS material.This socket is dirt resistant.
3. **2 ways 45\*45mm modules design:**2 way module socket that match Legrand Masic module socket.



**FZ-1770 outline drawing**



***Application***:****

