Wenzhou Safewire Electric CO.,Ltd.

**SPECIFICATION SHEET**

**PRODUCT NAME: IP66 waterproof socket for outdoor**

**PRODUCT No. :**  **SF66-S2S**





Address:2nd floor, Wealth Garden, Liushi town, Yueqing, Wenzhou,China ,325604

Tel:0086-577-61725369

Mob:0086-18612380398

ZIP:325604

（E-mail）：info@safewirele.com

(WEB): http://www.safewirele.com

**Specification**

|  |  |  |
| --- | --- | --- |
| 1 | Item | SF66-S2S |
| 2 | Type | Waterproof Switch Socket |
| 3 | Rated Voltage | 110V-250V |
| 4 | Rated Current | 13A |
| 5 | Material | ABS/PC |
| 6 | Color | Gray |
| 7 | Temperature | -20 ~ 55℃ |
| 8 | IP Grade | IP66 |
| 9 | Capacity | 2/duplex 45mm modules+Switch Socket |
| 10 | Outlet type | BS13A Socket; |
| 11 | Size | 300\*100\*73 |

**Product show**



**Feature**


1).IP66 Rated ,Cover will stay open to allow for easy access to sockets;

2).Applicable for the 45mm modules inside;Re-configuration is customization.

3). 300\*100mm dimension box of 4\*24mm knock out with transparent cover lid.

4).2\*UK socket with switch waterproof box

**Application**



The waterproof switch is suitable for the ports, shipping, cold storage, car washing and kitchen, bathroom, balcony, such as washing machines placed in damp or spray more environment,operation can be through the transparent membrane directly. Can be equipped with belt joint module series accessories and basic series; Framework can be installed in front of the fastening screw on the base of enough cable wiring space, make the installation Powder compact and reliable, convenient maintenance, ensure the protection grade is IP66 are closed.