**SPECIFICATION SHEET**

**PRODUCT NAME: Video connector sockets**

**PRODUCT No.:**  **F52D**

ADD: 152 xinguang industrial zone, yueqing city, zhejiang province

（TEL）:0086-577-62799688

（E-mail）：info@safewirele.com

(WEB): http://www.safewirele.c

**Quick Details**

Place of Origin:Zhejiang, China

Brand Name:OEM

Model Number:F52D

Type: modules socket

Grounding:Non-Grounding

Rated Voltage:110V-250V

Application:Residential / General-Purpose

Size:45\*22.5mm

Material:ABS

Color:White

**Product Show:**

|  |  |
| --- | --- |
| Panel Material: | ABS |
| Inside Material: | brass and ABS,metal holder |
| Color: | White |
| Voltage: | 110V--250V |
| Size | 22.5\*45mm |
| Type | Video connector sockets  |



**Application：**

Connect 3.5mm Male to 6.35mm Female（1/8" to 1/4" adapter）, allows you connect headphones to audio devices such as amplifiers or AV receivers with 6.35mm socket, widely work with earphone, headphone, karaoke system and etc and home audio equipment, such as amplifiers, mixing console,

home theater devices, amplifiers or AV receivers;

**Features:**

1.Connector : 3.5mm (1/8 Inch) Stereo Jack Male To 6.35mm (1/4 Inch) Stereo Jack Female,Mics and Headphones to be plugged into a 6.35mm(1/4) stereo jack socket input

2. Compatible headphones, sennheiser HD518 HD555 HD558 HD595 HD598 HD650 HD700 HD800, GRADO, AKG, audio-technical, Beyer dynamic, Sony etc.

3. Material:Made of Pure Copper wire inside

4.The new second generation colorful design, make life more exciting.

5.Pure copper connectors resist corrosion and ensure minimal signal loss.

6.360 degree grip treads help easy plugging and unplugging.

7. Made of solid brass copper, with a much longer service life compared with those plastic one.

**RoHS Certificate of Compliance：**Conforms with the Directive 2002/95/EC (ROHS) regarding to limitation of dangerous substances,in particular to clause 4 which forbids the use of substances: