**SPECIFICATION SHEET**

**PRODUCT NAME: HDMI sockets**

**PRODUCT No.:**  **H-HDMI-KSB**



ADD: 152 xinguang industrial zone, yueqing city, zhejiang province

（TEL）:0086-577-62799688

（E-mail）：info@safewirele.com

(WEB): http://www.safewirele.com

**Quick Details**

Place of Origin:Zhejiang, China

Brand Name:Safewire

Model Number:H-HDMI-KSB

Type:Twisted Pair, HDMI, Video Data Transmission, Audio Cables

Application:Speaker, Computer, Multimedia, Monitor, Telephone, DVD Player, Projector, HDTV, Camera, HOME THEATER

Connector Color:Black or White

Gender:Male-Male

Conductor:Bare Copper, 24-30AWG TC/BC/CCS, Gold Plated

Product name:HDMI 15mm cable

Material:ABS+pure Copper

Conductor material:99.9% pure oxgen free copper

Jacket Material:Nylon Mesh Braided Out-jacket

Function:Audio & Video Data Transmission

Voltage:300V DC,5MΩ/ 10ms

Working temperature:-25 to 80 degree Celsius

**Detail**

|  |  |  |
| --- | --- | --- |
| 1 | Type: | HDMI TO HDMI |
| 2 | Connector Type | Male-Male (optional) |
| 3 | Jacket | ABS+Nylon Braided |
| 4 | Connector Finish | 24K Gold plated |
| 5 | Plug | Zinc Alloy Housing |
| 6 | Cable | Round |
| 7 | Certification | ROHS, ISO9001, ISO14001, OHSAS18001 |
| 8 | HDTV TEST | TDR Test |
| 9 | Conductor | Oxygen Free Copper |
| 10 | Shielding | Triple layers |
| 11 | length | 1.5mm |

**Product Show:**





**Features:**

1.It supports HDMI 2.1 Data Rate up to 48Gbps, 8K60Hz, 4K120Hz

2.Backwards compatible with HDMI2.0/1.4, etc.

3.Supports uncompressed 8K video with Dynamic HDR.

4.Supports SDR, HDR, Dynamic HDR (HDR10+ and DV), ARC, e-ARC, VRR, ALLM, QTF, QMS

5.Supports HDCP1.4/2.2/2.3, CEC, 3D, Ethernet Channel, EDID.

6.Supports resolutions to 5K/100-120p 4:4:4 10Bit and 10K/24-30p 4:4:4 10Bit

**Application**: Monitor,TV,Computer,Media player, Mac, project, etc.

**RoHS Certificate of Compliance：**Conforms with the Directive 2002/95/EC (ROHS) regarding to limitation of dangerous substances,in particular to clause 4 which forbids the use of substances: