
**SPECIFICATION SHEET**

**PRODUCT NAME: speaker socket solder**

**PRODUCT No.:**  **F62A**



ADD: 152 xinguang industrial zone, yueqing city, zhejiang province

（TEL）:0086-577-62799688

（E-mail）：info@safewirele.com

(WEB): http://www.safewirele.com

**Quick Details**

Place of Origin:Zhejiang, China

Brand Name: Safewire

Model Number:F62A

Type: modules socket

Grounding:Non-Grounding

Rated Voltage:110V-250V

Rated Current:depends on modular

Application:Residential / General-Purpose

Size:45\*22.5mm

Material:ABS

Color:White

**Describe**

|  |  |
| --- | --- |
| Size | 45\*22.5mm |
| Material | ABS + Coupler |
| Color | white |
| Voltage | 110V-250V |
| Type | speaker socket solder |

**Product Show:**





**Feature**

Connector Type: Gold Plated Coupler or for use with wall plates or deksop socket or floor box

Speaker material: Hi Quality Gold Plated with solid core - provides excellent conductivity

Shell material: ABS

Fastening Type: For 4mm Banana plugs, Audio Spades or for bare audio wire via the Cross Holes

Colour Coded: Black colour printed detail

**Application:**  
    They are mainly used mobile phone, CD machine, wireless phone, digital notebook computer, digital camera, TV, home appliance, audio-visual, film and television and so on.

**RoHS Certificate of Compliance：**Conforms with the Directive 2002/95/EC (ROHS) regarding to limitation of dangerous substances,in particular to clause 4 which forbids the use of substances: